TUTORIAL AUTOGG

AutoGG
Do RGH&JTAG

# Table of Contents

- Description
- Rgh/Jtag using Flasher
- INSTALL XBOX APPS USING LAN
- QUICK OPEN NANDS MODE
- USB Cpukey&Nand Dumper
- Read only 1 mega with Flasher and inject to Full dump
- CHANGE TEMPERATURES
- CHANGE CONSOLE DATA
- Flash Nand using Raw Flash
- CREATE NEW IMAGE WITHOUT DUMP
- COM-Monitor
- Auto Update
  - Lan
  - Usb Dash
  - Usb Xell
- Auto Flash
- UPDATE AVATARS USING LAN
- LAN-FSD MODE ISSUES
- VideoTutorials
  - AutoGG Channel
  - drNefarious Channel
- Thanks

# DESCRIPTION

> AutogGG features:

> - Read Xbox Nand. It will Autodetect model |
> - Generate Nand to load Xell in console to obtain Cpukey. |
> - Once you have CpuKey.Generate Jtag / rgh (Glitch) / Retail, images - Flash generated Nand through Flasher (LPT/USB) or software (Xell or Dash) |
> - Change temperature sensors of console. |
> - Change console data: Serial, Reader Type (Osig), Region and dvdkey. |
> - Map / unmap Bad Blocks. |
> - Extract specific data from the console. - Create NandXell and Xebuild Images without Dump. | ____
> - Decrypt X-Val to check marks on console by Microsoft. - UnCripple to try to clear the console marks, - Console Nand Marks (Secdata) Check and Fix |
> - Read only 1Mb of Nand then read the rest through Xell and finally merge to get the full Nand much faster (Recommended for slow nands readers LPT) |
> - Nand File Explorer |
> - AutoUpdate Function |
> - Dash and Avatar Files Download |
> - Flash Glitch Chip (CPLD) USB&LPT |
> - Nandpro Manual Commands Window. - 3x Nands Compare. |
> - USB&FTP Xbox-Apps transfer (Freestyle, Homebrew, Emulators) |
> - Pc-Apps |
> - Available Online Data Server to store/retrieve your Cpukeys. . |
> - Images Viewer with many manufacturers chips , flasher .. |
> - Screen Captures ( InGame ) |

> - And more ...

Rgh/Jtag using Flasher

> > First you must know that to manage Nand of console have RISK OF BRICK
> > DO IT UNDER YOU RESPONSABILITY .
> > I am totally against the use of any method that violates copyright. This program is only developed to give the user the possibility to run free software, and ,in any case, the use of illegal software

> > 1. The program needs a dump (read) from nand console. We can get it in 3 ways :

> > * Reading nand using a Hard Nand reader(A) .
> > If you are using Flasher you need to select Model (A- Xflash, B-Squirter , C- Nandpro supported, D- MMC for Corona4G) , select port and Click Flasher>>Read
> > Try Nandpro Versions if you have problems. You can try Reset Configs. to solve issues.
> > AutoGG will try to detect the size of the Nand (if not detected select manually) then we ask how many read you want to make of your nand (2 recommended) and Size you want to read and then will proceed to make them and compared to ensure they are correct. Backups will be created.
> > * If your console has exploit you can get the dump through Net. Plug your local network (wireless or cable) and start Xell or FSD v3. Click IP-Xbox Read (C) to read it.Click CPUKEY (4) to decrypt .If everything is correct you will be prompted to save a copy of your encrypted data(5).

> > * If your console is already exploited you can dump your cpukey and nand to Usb. Click on Usb-Dumper button to prepare Device (some Usb devices need to be formated with Autogg), insert to console and boot Xell. Once dumped insert to PC to read and decrypt data.
> > [*]If you had already have the dump select it manually(B).[*]If nand has badblocks do not worry. Autogg will auto map them

> > 2. To generate Images autogg need cpukey of the console. If you have not it you will have to get it generating NandXell . To do this click Xell Create(1), and once generated Flash (2).

> > You need to program and install your chip selecting your correct file.Click Program Glitch and follow instructions..

> > Install your chip, in Help>Images you can view main schematics.

> > This will allow you to boot Xell.

> > Corona consoles have not Xell video on TV and in some cases Xell crashes. If you do not get Xell try to use any of the two alternatives Xell: blaKCat ( to get Cpukey using TV,Lan,Usb,Com-Monitor) or Mini (to get Cpukey using Usb)

> > Once Xell boots we obtain the Cpukey in several ways:

> > - Copy from the screen

> > - If you have the console connected to the network press CpuKey (4).

> > - Using Tutorial : "USB button Cpukey & Nand Dumper" described below.

> > - Using Tutorial: "Com-Monitor" described below.

> > Once you have introduced cpukey program automatically generate a file with the model name, serial number and cpukey to make a backup with all data.(5).

> > 3. With the correct cpukey we can build(7) Glitch JTAG or Retail images. Select Dash version and Options (6). In the case of Jtags you must select the Xell modelo and SMC you want to inject.

> > Once image is built you can flash Nand in several ways:

> > A-With Flasher (Hardware) >> Xebuild - Flash

> > B-Creating the necessary files on a USB (FAT32) and launch Xell with usb inserted. Raw Flash (8)

> > C-If we have Fsd v3 and console Lan connected . Ip-Flash (11)

> > 4.Once you have booted into the new Dash you could need to update (avatar. ..).
> > If Fsd v3 is booted and Lan connected you can FTP-Update Avatars. If its not so, Select USB to install files and insert it into the console. Boot it and update.

> AUTO-UPDATE:

> > AUTO-UPDATE (Lan Mode) :

> > At this moment for security is required internal Hdd or Usb connected to console to use this function

> > This function update your Nand trough Lan using a Usb Fat32 in glitched consoles with one-click:

> > SELECT DASH YOU WANT TO INTALL

> > CHECK LAN MODE AND CLICK DASH

> > READ PROMPT

> > AUTOGG WILL READ YOUR DUMP AND WILL CREATE NEW IMAGE .
> > THEN IT WILL BE FLASHED BUT CHECK PROMPT BEFORE.

> > CLICK YES TO FLASH IMAGE

> > WHEN FLASHED CONSOLE WILL REBOOT (UPDATED).

> > AUTOGG WILL ASK YOU TO UPDATE AVATARS (OPTIONAL)
> > YOU NEED IT TO USE KINECT

> > CLICK YES AND SYSTEMFILES WILL BE DOWNLOADED ...

> > ... AND FTP TRANSFERED TO CONSOLE

> > THEN CONSOLE WILL REBOOT

> > AND WILL PROMPT TO UPDATE, SELECT YES

> > DONE, YOUR CONSOLE DASH AND AVATARS ARE UPDATED

> > AUTO-UPDATE (Usb-Xell MODE) :

> > FIRST SELECT DASH VERSION YOU WANT TO INSTALL

> > CHECK USB MODE

> > READ PROMPT AND CONTINUE

> > CHOOSE XELL MODE (CORONA 4G NOT SUPPORTED )

> > CHOOSE USB DEVICE YOU WILL USE

> > YOU WILL BE PROMPT TO FORMAT YOUR USB DEVICE (RECOMMENDED)

> > IF YOU CLICK YES IT WILL BE FORMATED
> > IF YOU HAVE ERROR HERE TRY TO CLOSE WINDOWS FILE EXPLORER

> > AUTOGG WILL COPY FILES TO USB DEVICE . , THEN INSERT TO CONSOLE AND BOOT XELL

> > NAND & CPUKEY WILL BE SAVED TO USB DEVICE, THEN

> > INSERT IT BACK TO PC AND AUTOGG WILL READ DUMP AND WILL CREATE NEW UPDATED IMAGE .
> > ONCE DONE INSERT BACK TO CONSOLE AND IT WILL FLASH NEW IMAGE (RAW FLASH)

> > ONCE FLASHED AUTOGG WILL ASK YOU TO UPDATE AVATARS (OPTIONAL)
> > YOU NEED IT TO USE KINECT

> > CLICK YES AND SYSTEMFILES WILL BE DOWNLOADED ...

> > ... AND COPIED TO USB

> > GO TO OFFICIAL DASH AND INSERT USB ,IT WILL PROMPT TO UPDATE, SELECT YES

> > DONE, YOUR CONSOLE DASH AND AVATARS ARE UPDATED

> > AUTO-UPDATE (Modo Usb-Dash) :

> > > SELECT DASH VERSION YOU WANT TO INSTALL

> > CHECK USB MODE

> > READ WARNING

> > CHOOSE DASH MODE

> > SELECT USB DEVICE YOU WILL USE

> > YOU WILL BE PROMPT TO FORMAT YOUR USB DEVICE (RECOMMENDED)

> > IF YOU CLICK YES IT WILL BE FORMATED
> > IF YOU HAVE ERROR HERE TRY TO CLOSE WINDOWS FILE EXPLORER

> > THEN INSERT TO CONSOLE AND BOOT IT

> > YOUR NAND WILL BE SAVED TO USB THEN INSERT BACK TO PC AND CLICK OK

> > AUTOGG WILL READ AND CREATE UPDATE IMAGE.
> > BACKUPS WILL BE CREATED

> > READ WARNING

> > INSERT IT BACK TO CONSOLE AND CLICK A BUTTON TO FLASH NEW IMAGE

> > ONCE FLASHED AUTOGG WILL ASK YOU TO UPDATE AVATARS (OPTIONAL)
> > YOU NEED IT TO USE KINECT

> > CLICK YES AND SYSTEMFILES WILL BE DOWNLOADED ...

> > ... AND COPIED TO USB

> > GO TO OFFICIAL DASH AND INSERT USB ,IT WILL PROMPT TO UPDATE, SELECT YES

> > DONE, YOUR CONSOLE DASH AND AVATARS ARE UPDATED

> > Auto Flash
> > This method is being updated for next release.

> > This function will do one-click:
> > -Read nand, check and save backup in your nands folder.
> > -Create NandXell and flash it
> > -Once Xell boot cpukey will be save in Nand.
> > -Now you must Turn Off Console.
> > -Cpukey will be read from Nand trough Flasher , decrypted Nand and all Datas will be saved in a new folder created named with Serial.
> > -Create Xebuild Image and Flash it.
> > Done. If any Error Nand will be restored with backup.
> > Optional: After this functions you can create Usb to Update Avatars.

> Cpukey&Nand Dumper.
> (Read your dump using Usb)

* Insert Fat32 Usb device into PC.

* Press Nand USB Cpukey to prepare the device.

CHOOSE DASH MODE

SELECT YOUR USB DEVICE

YOU WILL BE PROMPT TO FORMAT YOUR USB DEVICE (RECOMMENDED)

IF YOU CLICK YES IT WILL BE FORMATED
IF YOU HAVE ERROR HERE TRY TO CLOSE WINDOWS FILE EXPLORER

THEN INSERT TO CONSOLE AND BOOT IT.

YOUR NAND WILL BE SAVED TO USB THEN INSERT BACK TO PC AND CLICK OK

INSERT IT BACK TO PC AND AUTOGG WILL READ DUMP

DONE!

## COM-Monitor

* We need to install a Com Port Reader. In the picture section you can see how you can use Squirter with only 2 wires soldered.

* Click NandXell - Com Monitor
* We will get a menu to config Com port.

* Boot Xell and you will see the Log of Xell .It will detect the CpuKey, Ip and Ldv of console.

* If we had loaded console Dump, it will decrypt it.

If something fails try another port configuration.

QUICK OPEN NANDS MODE :

New way to view and search our saved nands. Now will automatically backup all dumps we read.
Defaults folder: " autogg / nands / backups".
Once we get cpukey will save decrypted Nand And all specific Data in a new created folder named with Serial in your nands folder:
Default Folder "autogg / nands"
This folder can be changed at any time in Options (Select your nands folder)
Once selected Autogg will search for Valid Autogg Dumps and will Add them to NANDS Quick Open Menu .
In serial number search will open a new dialogue. If you edit the serial number field App will search (autogg format) nands containing all or part of the serial number in the Nands
Recent Files inlcuded.
If we deleted or copied new nands to folder manually click Update to Refresh
Click Reset to redo All Lists.

Read only 1 mega with Flasher and inject to Full dump ::
Este metodo es arriesgado por manipular la nand sin tener un backup completo

If you have a slow nand reader, the reading process can take hours.
There is the possibility of read-only area we need to generate the NandXell and once loaded in console then to read the rest of the Nand by Network
The process is as follows:
1-Press Read nand. Choose Size 1Meg. Save file.

AUTOGG WILL READ 1M

2-Choose image type (Glitch / JTAG) and click Generate NandXell.Once generated write it clicking Flash Xell. If all is ok start the console with network cable connected and chip installed. you will get the screen Xell
Read full dump now using Lan or Usb Dumper (read tutorial) . Load Full dump, you will get this warning.

You must inject first 1M dump from the beginning.

Done!

CHANGE TEMPERATURES:

In Nand are the parameters to regulate the temperature of CPU, GPU and Ram. The first 3 parameters are the objective temperatures by regulating the speed of the fans. The latter three parameters are the limit temperatures. If limit is exceeded the console shut down for protection.
To change these parameters only have to edit and click Change Temp button.
These will be stored and when we generate the image (Retail / Jtag / Glitch) shall apply the new parameters.
We must be careful with these option because if we set too much temperatures can burn the console . If we put too low fans will always be very fast and noise.

Load Dump and Autogg will show data.

Change Temperatures and Click Change Temps

Now you need to create new Xebuild Image and Flash it

You can check your new Temps launching DashLaunch.

Flash Nand using Raw Flash

Click Raw Flash and

select Usb Device .

Check files are copied to Usb, xenón.elf and nandflash.bin

Now click Ok and insert Usb to console and boot Xell, your Nand will be flashed.

CREATE NEW IMAGE WITHOUT DUMP :

If you have a Nand dump load it and try File-Extract to extract specific console data to folder. |
Rest Values clicking [X] or Menu File > Reset or restarting Autogg |
Select model and type of image and click RGH / JTAG - Create Image. |

We will see fields to fill:
Cpukey, SMC.bin, Keyvault.bin, smc-config.bin, ldv, badblocks.
To create an image you need at least Cpukey if you dont know it you need to create and flash Nandxell, boot Xell and get them using any method in this tutorial.
If you have specific data select them. LDV and Cpukey can be writen directly in their field.
If no Ldv selected image will have value 1. If any Data is not selected (smc, keyvault, smc.config) donors will be used.
Keyvault is needed for Retail

Create Xebuild image and Save it.

Finally once created Image if you havent used your Keyvault our new image wont have correct data .Load your xebuild image and edit data manually ,then create Final image, clicking Patch and Creating Xebuild Image |

_____________________________________________________________________________________________________________________________________________

INSTALL XBOX APPS USING LAN :

CLICK TO FIND YOUR CONSOLE.

SELECT APPS TO TRANSFER AND CLICK App>>>Ftp.

YOU WILL SEE TRANSFER PROCESS

ONCE FINISHED YOU CAN SCAN , ADD PATHS AND LAUNCH THEM FROM AUTOGG

_____________________________________________________________________________________________________________________________________________

UPDATE AVATARS USING LAN

CLICK TO FIND IP CONSOLE

AND CHECK YOUR DATA IN LOG

HERE YOU CAN SEE BLANK AVATARS. (BEFORE PROCESS)

SELECT SAME DASH YOU HAVE INSTALLED , CHECK LAN MODE AND CLICK AVATARS

SYSTEMFILES WILL BE DOWNLOADED ...

... AND FTP TRANSFERED TO CONSOLE

THEN CONSOLE WILL REBOOT

AND WILL PROMPT TO UPDATE, SELECT YES

DONE, YOUR CONSOLE AVATARS ARE UPDATED

HOW TO MODIFY YOUR CONSOLE DATA :

You have the option to modify the console data: Num.Serie, type reader (Osig), Region and dvdkey.

Just load your nand and modify data. Click on Patch then on Xebuild >> Create and new Xebuild image will be created . Now you can load and flash it or directly click on Raw-Flash USB to write through Xell.

LAN MODE ISSUES :

- If you have any errors in process check:

* Some antivirus block FTP communication between PC (AUtogg) and the console, try to disable it, uninstall it or use another PC.
* The option "Do not scan at StartUP" within FSD settings should not be marked.
* Fsd v3 or later is requireed , you can create it using XboxApps>>USB-Apps and boot console with the USB inserted .
* Autogg needs to find Ip console, if you have subnets it wont work.
* After updating the Dash in some cases Avatars Update >> Lan mode is not supported and gives an error on console. Upgrade Avatars using USB method.

If you have problems with this mode use the classic USB method or follow tutorial to use manual mode .

Thanks:
A los Betatesters especialmente a breily, MBTecnic, Spainsellers, Console Open,
Logic Sunrise, Casca ,Mac1512 ,segiolc, Rogero y foro EOL.

Devs:GLIGLI, Tiros, Fsd Team, Xebuild team, cOz, Squirt Team, Swizzy, Juvenal
Lenguajes:
Dennn : Ruso
wiiallgarant , Artik , Razkar: Frances
Federause, Marco(ConsoleOpen), Squirt Team: Italiano
Kalel(darth Vader, cursos games,Niceshoot):Português
Creadores Xbox Apps linkadas
Traducción FSD por bocasecaman
Logic-Sunrise :servidor Web Autogg

Everyone involved..