// Created using Xilinx Cse Software [ISE - 14.7]
// Date: Tue Jan 21 10:44:39 2014

TRST OFF;
ENDIR IDLE;
ENDDR IDLE;
STATE RESET;
STATE IDLE;
FREQUENCY 1E6 HZ;
//Operation: Program -p 0 -e -v -r -u 87654321 
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (01) SMASK (ff) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f6e5f093) MASK (0fff8fff) ;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (03) ;
//Boundary Scan Chain Contents
//Position 1: xc2c64a
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'idcode' instruction.
SIR 8 TDI (01) ;
SDR 32 TDI (00000000) TDO (f6e5f093) ;
//Check for Read/Write Protect.
SIR 8 TDI (ff) TDO (01) MASK (03) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
// Loading devices with 'enable' or 'bypass' instruction.
SIR 8 TDI (e8) ;
// Loading devices with 'erase' or 'bypass' instruction.
ENDIR IRPAUSE;
SIR 8 TDI (ed) SMASK (ff) ;
ENDIR IDLE;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRPAUSE;
RUNTEST DRPAUSE 20 TCK;
STATE  IDLE;
RUNTEST IDLE 100000 TCK;
STATE  DRPAUSE;
RUNTEST DRPAUSE 5000 TCK;
RUNTEST IDLE 1 TCK;
// Loading devices with 'init' or 'bypass' instruction.
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IDLE;
RUNTEST IDLE 20 TCK;
// Loading devices with 'init' or 'bypass' instruction.
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRUPDATE IDLE;
RUNTEST 800 TCK;
ENDIR IDLE;
// Loading devices with 'conld' or 'bypass' instruction.
SIR 8 TDI (c0) ;
RUNTEST 100 TCK;
// Loading devices with 'conld' or 'bypass' instruction.
SIR 8 TDI (c0) ;
RUNTEST 100 TCK;
// Loading devices with 'enable' or 'bypass' instruction.
SIR 8 TDI (e8) ;
// Programming.
// Loading devices with 'program' instruction.
ENDIR IRPAUSE;
SIR 8 TDI (ea) ;
SDR 281 TDI (0003c1ffffffffffffbf7ffffffffffffffffe7c7bffffffffaf537fbcabb5bf4cfffe0f) SMASK (01ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
ENDIR IDLE;
RUNTEST 10000 TCK;
SDR 281 TDI (0102f9ffffffffffffbf7ffffffffffffffffe7e73ffffffffffffffffffffffffeffe7f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01828fffffffffffffbf7ffffffffffffffffe7e6ceeeeeeeeeffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0083c1ffffffffffffbf7ffffffffffffffffe7e3ceeeeeeeeefffffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00c3f9fffffffffff7bffffffffffffffffffe7e73fffffffffffffffffffffffff7feef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01c0f9fffffffffff7bffffffffffffffffffe7e3dfffffffffffffffffffffffffede7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0143c1ffffffffffffbf7ffffffffffffffffe5e6fffffffffffffffffffffffffff5e0f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0042f9dfffffffffffff7dfffffbfffffffffe7e79ffffffffffffffffffffffffeffe67) ;
RUNTEST 10000 TCK;
SDR 281 TDI (006289ffffffffffffbf7ffffffffffffffffe7e6ceeeeeeeeeffffffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0163c1fffffffffff7bffffffffffffffffffe7e73ffffffffffffffffffffffffff3e0f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01e398bffffffffffffffbfffffbfffffffffe5e6ffffffffffffffaffeffbfffffffe67) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00e2fdf5ad32bdd7fdf7effcff36b77bfdfffe787fffffaeeeeff4fedfd2bcf54dfffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00a3c1fffffffffff7bffffffffffffffffffe7c6fffffffaeef52ab4af55f5552ffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01a3997fffffffffffff7bfffffffffffffffe5e6fffffffffffffffffffffcffffff2ef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0122fdfffffcbfbf7fffff7ffffffd7ffffffe3e5eeeeeeeeeeffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0023c1fffffffffff7bffffffffffffffffffe7c3fffafffffffff57ffcebbf4dfffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (003399f7eff7f76bff6bcfbb3fff3fddbdfffe7a77ffffffffffffffffffffffffffecef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0132fdf3f777f773fb7dbfff7fef6fd7fdfffe787ffffffffffb73dffebceeaaed7ffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01b3c17ffffffffffffefbfffffffffffffffe7c6ffffbffffffffffffff5df5bcffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00b3993fffffffffffff7dfffffffffffffffe7e1fffffffffffffffffffffffffeffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00f2fdfffffffffffaebaeaaabfffffffffffffffebffffffffffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01f3dbebaaaaaaaebfffffffffffffffffffffffffffffffffff555555554aaaaaffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0173d9fffffffffffffffffffffffffffffffffffff4bffffffffffffffffffffffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0072fdffffffffffffffffffffffffffffffe1e7fffff4bffffffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0053c1fffffffffffffffffffffffffffffffffffffffff4bfffffffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0153f95fffffffffffffffffffffffffffffffffffffffffebffffffffffffffffd7feef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01d0f9ffffffffffffffffffff4eaaabbfffffffffffffffff4bfffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00d3c1ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff4b6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0093f9f7adecd5f6fcf7cfb53fef5dd5bdfffe7a5f3333333333fffffffffffffffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0190f9fffffffffff7bffffffffffffffffffe763fffffffffff5552aabfeffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0113c1fffffffffff7bffffffffffffffffffe763faeeeeeeeeffffffffffffffffffe0f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0013f9fffffff54effffffd2bfffffcbbffffeeefffffffffffffffffffffffffffffe67) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0018f9f3ad4ab4cf7d75d7555feeaaabbdfffefafffffffffffffffffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (011bdbfffffffffff7bffffffffffffffffffefebfffffffffffffffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0198f9fffffffffffffffffffdfffffffffffe6c7ffaeeeeeeeffffffffffffffffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (009a8bfffffffffffffdffbfdffff7ffdffffe3c7ffffffaeeef555555555555557ffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00dbc1fbdffd3fff7ffffffffedffdaf7ffffefaffffffffffffffffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01db99fdbfdabffffffffffffeffdfeb7ffffe727ffffeeeeeeebffbcbffff7ffffffe8d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (015af9ffffffffffdffffffffffffffffffffe6e5eeeeeeeeeeffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (005bc1ffffffffffffbffffffffffffffffffe367f7777777777ffffffffffffffffeb6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (007b99ffffffffffffffffffffffffffffffff7d7ffffffffaefdff7cebaeebddffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (017af9f5d557d5577f75d6b73ff7557bddfffefafffffffffffffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01fbc1fffd2fff7fffffaff7ffffafffddfffeeefffffffffffffffffffffffffffffe0f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00fb99fffffffffffffffffff7fffffffffffeeefffffffffffffffffffffffffffffe67) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00bafdfffffffffffffffffffffffffffff5ff7fffffffffffffffffffffffffffff3e7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01bbc1ffffffffffffff7ffffffffffffffffe3e7ceeeeeeeeeffffffffffffffffffe0f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (013b99ffffffffffffbf7ffffffffffffffffe5e6fffffffffffffffffffffffffbffe67) ;
RUNTEST 10000 TCK;
SDR 281 TDI (003afdff7ffffffffffffffffffffffffff99e7ffffffffffffffffffffffffffffbfe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (002bd9ffdddf7df7df7dfffffffffffffffffe7e78ffffffbdefdbf7fffedffcefffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (012bddffffffffffffffffdbeffffffffffffe667fffffffffffffffffffffffdddf77ef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01a8f9ffff5f7ffffffffffffffffffffffffe7e6dfffffffffffffffffffffffefffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00abd9fff5df7ffffffffffffffffffffffffe7e3dfffffffffffffffffffffffbefff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00ebd9bbbbbefbefbefaff7ffefbfffffffffe7e6cfffffffffffcbffffffffffffffe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01e8f9ffffffffffffffdffffffffffffffffe7e3defff3fffffffffcbfffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (016bd9f3dddf7df7df7dfffffffffffffffffe5e6ff75557ffffffffcf75ffefffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (006bd9bddddf7df7df7cff7ffefbfffffffffe7e79eff6bbaaeeababbacaaebafffffe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (004af9fffffff7fffffffffffffffffffffffe7e6dfffffffffffffffffffffffbbefa7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (014bd9fffffffdf7df7dfffffffffffffffffe7e797fffffb7fffbffffff2bffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01cbdd7ffffffffffffffffffffffffffffffefeeffffffffffffffffffffffffffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00caf9ffffffffffffffffffffffffffffffff7f76ffffffbf6ff3fdfffef7fb7ffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (008bd9fffffffdf7df7dfffffffffffffffffe7e66ffffffcabffbffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (018bddbddddf7df7df7cff7ffefbfffffffffe7e67f7fbef2aeeababddbcaebafffffe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (010af9ffffffffffffffffff7ffffffffffffe7e37fbfffffffffffffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (000bd9fffffffffffff5fffffffffffffffffe7e36ffffffffffffffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (000ec5ffffffffffffffffdbf7fffffffffffe7e1ffffffffffffffffffffffffbbeee6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (010ef9fffffd7ffffffffffffffffffffffffe7e677ffffffffffffffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (018fd9ffffffffd7df7dfffffffffffffffffe7e37f7bf5bd57755d5ddef57cd7fffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (008cfbbddddf7df7df7cf7fffefbfffffffffe7e1fef7ebbaaeeababbbeeaf7afffffe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00ce89ffffffffffffffffdcefffffffffffffffffcaabfffffffffffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01cfd9fffffffffffffdceffffffffffffffffffffffff557ffffffffffffeafffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (014fddffffffffffdcefffffffffffffffffffffffffffffd55ffffffffffffaeffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (004ef9bfd7fffffffffffffffffffffffffffffffffffffffff557fffffffffffafffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (006fd9fffffffdcefffffffffffffffffffffffffffffffffffffaabffffffffffd7ff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (016fdcfffffffffffffffffffffffffffffff9ffffffffffffffffff55fffffffffebeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01eef9ffffdcefffffffffffffffffffffffffffffffffffffffffffff55ffffffffea7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00efd9f5faffffffffffffffffffffffffffffffffffffffffffffffffff55ffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00afddffffffffffffffffbb6ffffffffffffe7e3dfffffffffffffffffffffffbbfbe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01aef9ffffffffff5f7dfffffffffffffffffe7e1f7ffffffffffbfffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (012fdfffffffffffffffeffffffffffffffffe3e5f7ffffffffffbffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (002cffffdddf7ffffffffffffffffffffffffe3e5f7ffffffffffffffffffffffffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (003c01ffffffffffffffffffffffffffffffff7f5f7ffffffffffbfffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (013fdffffffffffffd7dfffffffffffffffffe7e1f7ffffffffffbffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01bcddffffffffffffffffffffffffffffffff7f777ffffffffffffffffffffffffffeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00be05fffff7df7df7dffdf7dffff7df7dfbbe7f5ffffffffffffffffffffffffccf327c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00ffd9ffffffffffffffffffffffffffffffff7f5efffffffffffbffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01ffddf3bbbefbefbefbfffffffffffffffffe1e7fffffffd533fcffffff53fd6ffffe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (017ef9ffeefbefbefbefbffffffffffffffffe7a7d7ffffffff2affffffffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (007fd9ffffffffffffffff7ffffffffffffffe787ff3ff52fffffffeff3ffebfffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (005fddffffffffffffffffffffffffffffffff7f5ffffffffffffffffffffffffbbeeeef) ;
RUNTEST 10000 TCK;
SDR 281 TDI (015ef9bf7ffffffffffffffffffffffffffafefffffffffffffffffffffffffffffffe7c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (01dfd9ffffffffffffffffffffffffffffffff5f7fbfffffffffffffffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (00dec5fffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffe6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (009ef9fffffffffffffffffffffffffffff5ff7ffffeaadfffffffffbdfffffffffffe7d) ;
RUNTEST 10000 TCK;
SDR 281 TDI (019fd9ffffffffffffffffffffffffffffffff5f7fffffffffef7fcbffffffffffffff6f) ;
RUNTEST 10000 TCK;
SDR 281 TDI (011fd9fffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffe1c) ;
RUNTEST 10000 TCK;
SDR 281 TDI (001ef9ffdddf7ffffffffffffffffffffffdde7efbfffffffffffffffffffffffffbff45) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0017ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 10000 TCK;
SDR 281 TDI (0117ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 10000 TCK;
// Loading devices with 'init' or 'bypass' instruction.
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IDLE;
RUNTEST IDLE 20 TCK;
// Loading devices with 'init' or 'bypass' instruction.
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRUPDATE IDLE;
RUNTEST 800 TCK;
ENDIR IDLE;
// Loading devices with 'conld' or 'bypass' instruction.
SIR 8 TDI (c0) ;
RUNTEST 100 TCK;
// Loading devices with 'conld' or 'bypass' instruction.
SIR 8 TDI (c0) ;
RUNTEST 100 TCK;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
//Loading device with 'enable' instruction.
SIR 8 TDI (e8) ;
//Loading device with 'enable' instruction.
SIR 8 TDI (e8) ;
// Verification. 
// Loading device with a 'verify' instruction. 
ENDIR IRPAUSE;
SIR 8 TDI (ee) ;
ENDDR DRPAUSE;
SDR 7 TDI (00) SMASK (7f) ;
ENDIR IDLE;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1ffffffffffffbf7ffffffffffffffffe7c7bffffffffaf537fbcabb5bf4cfffe0f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (40) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffffffffffffbf7ffffffffffffffffe7e73ffffffffffffffffffffffffeffe7f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (60) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (028fffffffffffffbf7ffffffffffffffffe7e6ceeeeeeeeeffffffffffffffffffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (20) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1ffffffffffffbf7ffffffffffffffffe7e3ceeeeeeeeefffffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (30) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03f9fffffffffff7bffffffffffffffffffe7e73fffffffffffffffffffffffff7feef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (70) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9fffffffffff7bffffffffffffffffffe7e3dfffffffffffffffffffffffffede7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (50) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1ffffffffffffbf7ffffffffffffffffe5e6fffffffffffffffffffffffffff5e0f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (10) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9dfffffffffffff7dfffffbfffffffffe7e79ffffffffffffffffffffffffeffe67) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (18) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0289ffffffffffffbf7ffffffffffffffffe7e6ceeeeeeeeeffffffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (58) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fffffffffff7bffffffffffffffffffe7e73ffffffffffffffffffffffffff3e0f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (78) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0398bffffffffffffffbfffffbfffffffffe5e6ffffffffffffffaffeffbfffffffe67) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (38) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdf5ad32bdd7fdf7effcff36b77bfdfffe787fffffaeeeeff4fedfd2bcf54dfffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (28) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fffffffffff7bffffffffffffffffffe7c6fffffffaeef52ab4af55f5552ffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (68) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03997fffffffffffff7bfffffffffffffffe5e6fffffffffffffffffffffcffffff2ef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (48) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdfffffcbfbf7fffff7ffffffd7ffffffe3e5eeeeeeeeeeffffffffffffffffffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (08) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fffffffffff7bffffffffffffffffffe7c3fffafffffffff57ffcebbf4dfffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (0c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0399f7eff7f76bff6bcfbb3fff3fddbdfffe7a77ffffffffffffffffffffffffffecef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (4c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdf3f777f773fb7dbfff7fef6fd7fdfffe787ffffffffffb73dffebceeaaed7ffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (6c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c17ffffffffffffefbfffffffffffffffe7c6ffffbffffffffffffff5df5bcffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (2c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03993fffffffffffff7dfffffffffffffffe7e1fffffffffffffffffffffffffeffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (3c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdfffffffffffaebaeaaabfffffffffffffffebffffffffffffffffffffffffffe7c) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (7c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03dbebaaaaaaaebfffffffffffffffffffffffffffffffffff555555554aaaaaffff6f) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (5c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffffffffffffffffffffffffffffffff4bffffffffffffffffffffffffeef) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (1c) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdffffffffffffffffffffffffffffffe1e7fffff4bffffffffffffffffffffffe7c) MASK (
03fffffffffffffffffffffffffffffe001ff801ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (14) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fffffffffffffffffffffffffffffffffffffffff4bfffffffffffffffffffff6f) MASK (
03fffffffffffffffffffffffffffffe001f8001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (54) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03f95fffffffffffffffffffffffffffffffffffffffffebffffffffffffffffd7feef) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (74) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9ffffffffffffffffffff4eaaabbfffffffffffffffff4bfffffffffffffffffe7c) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (34) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff4b6f) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (24) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03f9f7adecd5f6fcf7cfb53fef5dd5bdfffe7a5f3333333333fffffffffffffffffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (64) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9fffffffffff7bffffffffffffffffffe763fffffffffff5552aabfeffffffffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (44) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fffffffffff7bffffffffffffffffffe763faeeeeeeeeffffffffffffffffffe0f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (04) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03f9fffffff54effffffd2bfffffcbbffffeeefffffffffffffffffffffffffffffe67) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (06) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9f3ad4ab4cf7d75d7555feeaaabbdfffefafffffffffffffffffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (46) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03dbfffffffffff7bffffffffffffffffffefebfffffffffffffffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (66) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9fffffffffffffffffffdfffffffffffe6c7ffaeeeeeeeffffffffffffffffffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (26) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (028bfffffffffffffdffbfdffff7ffdffffe3c7ffffffaeeef555555555555557ffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (36) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fbdffd3fff7ffffffffedffdaf7ffffefaffffffffffffffffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (76) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0399fdbfdabffffffffffffeffdfeb7ffffe727ffffeeeeeeebffbcbffff7ffffffe8d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (56) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffffffffffdffffffffffffffffffffe6e5eeeeeeeeeeffffffffffffffffffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (16) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1ffffffffffffbffffffffffffffffffe367f7777777777ffffffffffffffffeb6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (1e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0399ffffffffffffffffffffffffffffffff7d7ffffffffaefdff7cebaeebddffffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (5e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9f5d557d5577f75d6b73ff7557bddfffefafffffffffffffffffffffffffffffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (7e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1fffd2fff7fffffaff7ffffafffddfffeeefffffffffffffffffffffffffffffe0f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (3e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0399fffffffffffffffffff7fffffffffffeeefffffffffffffffffffffffffffffe67) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (2e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdfffffffffffffffffffffffffffff5ff7fffffffffffffffffffffffffffff3e7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (6e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03c1ffffffffffffff7ffffffffffffffffe3e7ceeeeeeeeeffffffffffffffffffe0f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (4e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0399ffffffffffffbf7ffffffffffffffffe5e6fffffffffffffffffffffffffbffe67) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (0e) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02fdff7ffffffffffffffffffffffffff99e7ffffffffffffffffffffffffffffbfe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (0a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9ffdddf7df7df7dfffffffffffffffffe7e78ffffffbdefdbf7fffedffcefffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (4a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ddffffffffffffffffdbeffffffffffffe667fffffffffffffffffffffffdddf77ef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (6a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9ffff5f7ffffffffffffffffffffffffe7e6dfffffffffffffffffffffffefffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (2a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fff5df7ffffffffffffffffffffffffe7e3dfffffffffffffffffffffffbefff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (3a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9bbbbbefbefbefaff7ffefbfffffffffe7e6cfffffffffffcbffffffffffffffe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (7a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00f9ffffffffffffffdffffffffffffffffe7e3defff3fffffffffcbfffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (5a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9f3dddf7df7df7dfffffffffffffffffe5e6ff75557ffffffffcf75ffefffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (1a) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9bddddf7df7df7cff7ffefbfffffffffe7e79eff6bbaaeeababbacaaebafffffe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (12) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9fffffff7fffffffffffffffffffffffe7e6dfffffffffffffffffffffffbbefa7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (52) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffdf7df7dfffffffffffffffffe7e797fffffb7fffbffffff2bffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (72) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03dd7ffffffffffffffffffffffffffffffefeeffffffffffffffffffffffffffffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (32) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffffffffffffffffffffffffffffffff7f76ffffffbf6ff3fdfffef7fb7ffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (22) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffdf7df7dfffffffffffffffffe7e66ffffffcabffbffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (62) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ddbddddf7df7df7cff7ffefbfffffffffe7e67f7fbef2aeeababddbcaebafffffe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (42) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffffffffffffffffff7ffffffffffffe7e37fbfffffffffffffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (02) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffffffff5fffffffffffffffffe7e36ffffffffffffffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (03) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02c5ffffffffffffffffdbf7fffffffffffe7e1ffffffffffffffffffffffffbbeee6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (43) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9fffffd7ffffffffffffffffffffffffe7e677ffffffffffffffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (63) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9ffffffffd7df7dfffffffffffffffffe7e37f7bf5bd57755d5ddef57cd7fffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (23) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00fbbddddf7df7df7cf7fffefbfffffffffe7e1fef7ebbaaeeababbbeeaf7afffffe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (33) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0289ffffffffffffffffdcefffffffffffffffffcaabfffffffffffffffffffffffe7d) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (73) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffffffffdceffffffffffffffffffffffff557ffffffffffffeafffffff6f) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (53) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ddffffffffffdcefffffffffffffffffffffffffffffd55ffffffffffffaeffffeef) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (13) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9bfd7fffffffffffffffffffffffffffffffffffffffff557fffffffffffafffe7c) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (1b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffdcefffffffffffffffffffffffffffffffffffffaabffffffffffd7ff6f) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (5b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03dcfffffffffffffffffffffffffffffff9ffffffffffffffffff55fffffffffebeef) MASK (
03fffffffffffffffffffffffffffffe00078001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (7b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffffdcefffffffffffffffffffffffffffffffffffffffffffff55ffffffffea7c) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (3b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9f5faffffffffffffffffffffffffffffffffffffffffffffffffff55ffffffff6f) MASK (
03fffffffffffffffffffffffffffffe00000001ffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (2b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ddffffffffffffffffbb6ffffffffffffe7e3dfffffffffffffffffffffffbbfbe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (6b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffffffffff5f7dfffffffffffffffffe7e1f7ffffffffffbfffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (4b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03dfffffffffffffffeffffffffffffffffe3e5f7ffffffffffbffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (0b) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00ffffdddf7ffffffffffffffffffffffffe3e5f7ffffffffffffffffffffffffffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (0f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0001ffffffffffffffffffffffffffffffff7f5f7ffffffffffbfffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (4f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03dffffffffffffd7dfffffffffffffffffe7e1f7ffffffffffbffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (6f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (00ddffffffffffffffffffffffffffffffff7f777ffffffffffffffffffffffffffeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (2f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (0205fffff7df7df7dffdf7dffff7df7dfbbe7f5ffffffffffffffffffffffffccf327c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (3f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9ffffffffffffffffffffffffffffffff7f5efffffffffffbffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (7f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ddf3bbbefbefbefbfffffffffffffffffe1e7fffffffd533fcffffff53fd6ffffe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (5f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffeefbefbefbefbffffffffffffffffe7a7d7ffffffff2affffffffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (1f) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9ffffffffffffffff7ffffffffffffffe787ff3ff52fffffffeff3ffebfffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (17) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ddffffffffffffffffffffffffffffffff7f5ffffffffffffffffffffffffbbeeeef) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (57) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9bf7ffffffffffffffffffffffffffafefffffffffffffffffffffffffffffffe7c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (77) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9ffffffffffffffffffffffffffffffff5f7fbfffffffffffffffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (37) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02c5fffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffe6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (27) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9fffffffffffffffffffffffffffff5ff7ffffeaadfffffffffbdfffffffffffe7d) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (67) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9ffffffffffffffffffffffffffffffff5f7fffffffffef7fcbffffffffffffff6f) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (47) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03d9fffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffe1c) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (07) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (02f9ffdddf7ffffffffffffffffffffffdde7efbfffffffffffffffffffffffffbff45) MASK (
03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (05) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) MASK (
0000000000000000000000000000000000000000000000000000000000000000000000) ;
RUNTEST 100 TCK;
ENDDR DRPAUSE;
SDR 7 TDI (45) SMASK (7f) ;
RUNTEST DRPAUSE 20 TCK;
ENDDR IDLE;
RUNTEST IDLE 100 TCK;
// masking lower UES bits. 
SDR 274 TDI (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) SMASK (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) TDO (03ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) MASK (
0000000000000000000000000000000000000000000000000000000000000000000000) ;
RUNTEST 100 TCK;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IDLE;
RUNTEST IDLE 20 TCK;
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRUPDATE IDLE;
RUNTEST 800 TCK;
ENDIR IDLE;
//Loading device with 'conld' instruction.
SIR 8 TDI (c0) ;
RUNTEST IDLE 100 TCK;
//Loading device with 'enable' instruction.
SIR 8 TDI (e8) ;
// Loading device with a 'program' instruction. 
ENDIR IRPAUSE;
SIR 8 TDI (ea) ;
SDR 281 TDI (0117ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff87654321) SMASK (01ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
ENDIR IDLE;
RUNTEST 10000 TCK;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IDLE;
RUNTEST IDLE 20 TCK;
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRUPDATE IDLE;
RUNTEST 800 TCK;
ENDIR IDLE;
//Loading device with 'enable' instruction.
SIR 8 TDI (e8) ;
// Setting Done bit ... 
// Loading device with a 'program' instruction. 
ENDIR IRPAUSE;
SIR 8 TDI (ea) ;
SDR 281 TDI (0017fdffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
ENDIR IDLE;
RUNTEST 10000 TCK;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IDLE;
RUNTEST IDLE 20 TCK;
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRUPDATE IDLE;
RUNTEST 800 TCK;
ENDIR IDLE;
//Loading device with 'enable' instruction.
SIR 8 TDI (e8) ;
// Loading device with a 'program' instruction. 
ENDIR IRPAUSE;
SIR 8 TDI (ea) ;
SDR 281 TDI (001555ffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffffff) ;
ENDIR IDLE;
RUNTEST 10000 TCK;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IDLE;
RUNTEST IDLE 20 TCK;
ENDIR IRPAUSE;
SIR 8 TDI (f0) SMASK (ff) ;
STATE  IREXIT2 IRUPDATE DRSELECT DRCAPTURE DREXIT1 DRUPDATE IDLE;
RUNTEST 800 TCK;
ENDIR IDLE;
//Loading device with 'conld' instruction.
SIR 8 TDI (c0) ;
RUNTEST IDLE 100 TCK;
//Loading device with 'idcode' instruction.
SIR 8 TDI (01) ;
SDR 32 TDI (00000000) SMASK (ffffffff) TDO (f6e5f093) MASK (0fff8fff) ;
//Check for Done bit.
SIR 8 TDI (ff) TDO (05) MASK (07) ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
HDR 0 ;
TDR 0 ;
TIR 0 ;
HIR 0 ;
TDR 0 ;
HDR 0 ;
SIR 8 TDI (ff) ;
SDR 1 TDI (00) SMASK (01) ;
